DATATYPE = CDS STUDY DEFINITION
FILENAME = /eofcs/data/plan/database/export/network_65.def
INSTRUME = CDS
DATE_CRE = 2003/03/17 23:21:28
END

LINELIST
    LL_ID    = 430
    DETECTOR = N
    LL_DESC  = Chromospheric Network 6
    N_LINES  = 6
    LL_IND   = 1
        LINENAME = O III
        WAVELNTH = 525.796
        GR_ORDER = 1
        CEN_PIX  = 122
        WAVEBAND = 2
    LL_IND   = 2
        LINENAME = O IV-1
        WAVELNTH = 552.877
        GR_ORDER = 1
        CEN_PIX  = 354
        WAVEBAND = 2
    LL_IND   = 3
        LINENAME = O IV-2
        WAVELNTH = 556.031
        GR_ORDER = 1
        CEN_PIX  = 381
        WAVEBAND = 2
    LL_IND   = 4
        LINENAME = Ne VI
        WAVELNTH = 562.925
        GR_ORDER = 1
        CEN_PIX  = 440
        WAVEBAND = 2
    LL_IND   = 5
        LINENAME = O III
        WAVELNTH = 599.51
        GR_ORDER = 1
        CEN_PIX  = 753
        WAVEBAND = 2
    LL_IND   = 6
        LINENAME = O  V
        WAVELNTH = 629.623
        GR_ORDER = 1
        CEN_PIX  = 1009
        WAVEBAND = 2

DATAWIN
    DW_ID    = 558
    DETECTOR = N
    DW_DESC  = Background,   6 lines. {0}  dex = (29,120) pixels <20639>
    W_WIDTH  = 29
    W_HEIGHT = 120
    VDS_BACK = 1
    LL_ID    = 430
    N_WINS   = 10
    DW_IND   = 1
        WIN_NAME = O_3_525_80                              
        WIN_DEF  = (108,392,29,120)
        WIN_FLAG = 0
    DW_IND   = 2
        WIN_NAME = WW_552_88                               
        WIN_DEF  = (340,392,29,120)
        WIN_FLAG = 0
    DW_IND   = 3
        WIN_NAME = WW_556_03                               
        WIN_DEF  = (367,392,29,120)
        WIN_FLAG = 0
    DW_IND   = 4
        WIN_NAME = Ne_6_562_92                             
        WIN_DEF  = (426,392,29,120)
        WIN_FLAG = 0
    DW_IND   = 5
        WIN_NAME = O_3_599_51                              
        WIN_DEF  = (739,392,29,120)
        WIN_FLAG = 0
    DW_IND   = 6
        WIN_NAME = O_5_629_62                              
        WIN_DEF  = (995,392,28,120)
        WIN_FLAG = 0
    DW_IND   = 7
        WIN_NAME = Background                              
        WIN_DEF  = (20,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 8
        WIN_NAME = Background                              
        WIN_DEF  = (994,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 9
        WIN_NAME = Background                              
        WIN_DEF  = (20,994,10,10)
        WIN_FLAG = 0
    DW_IND   = 10
        WIN_NAME = Background                              
        WIN_DEF  = (994,994,10,10)
        WIN_FLAG = 0

RASTER
    RAS_ID   = 10
    DETECTOR = N
    RAS_DESC = Slit(2x240),Posns(120,-)@(2,-) steps
    SLIT_NUM = 4
    XSTEP    = 2
    YSTEP    = 0
    NX       = 120
    NY       = 1

RASTER_VAR
    RAS_ID   = 10
    RAS_VAR  = 73
    RV_DESC  = (240x240) arcsec, 25s <QUIET>  Comp. 2 IDs-(430,558)
    EXPTIME  = 25
    LL_ID    = 430
    COMP_ID  = 2
    COMP_OPT = 0
    DW_ID    = 558
    IEF_ID   = 0
    VDS_ORIENT = 0
    VDS_MAP  = 2
    TEL_RATE = M
    DURATION = 3748
    USABLE   = Y

STUDY
    STUDY_ID = 10
    TITLE_ID = 137
    OBS_PROG = NETWORK
    TITLE    = CHROMOSPHERIC NETWORK  4'X4'
    CATEGORY = S
    VAR_POINT = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 10
        POINTING = 1
        INS_X    = 0
        INS_Y    = 0

STUDY_VAR
    STUDY_ID = 10
    TITLE_ID = 137
    STUDYVAR = 65
    SV_DESC  = 25 S, TR + NE VI - 6 WINDOWS, 29 PIXEL
    N_RASTERS0 = 0
    DURATION0 = 0
    DURATION1 = 3748
    ZONE_ID  = 4
    USABLE   = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 10
        RAS_VAR  = 73
        N_REPEAT_R = 1
