DATATYPE = CDS STUDY DEFINITION
FILENAME = /eofcs/data/plan/database/export/sas250w_12.def
INSTRUME = CDS
DATE_CRE = 2003/04/30 14:45:28
END

LINELIST
    LL_ID    = 440
    DETECTOR = N
    LL_DESC  = Bright AR Upper TR
    N_LINES  = 6
    LL_IND   = 1
        LINENAME = O IV
        WAVELNTH = 554.52
        GR_ORDER = 1
        CEN_PIX  = 368
        WAVEBAND = 2
    LL_IND   = 2
        LINENAME = Ca X
        WAVELNTH = 557.765
        GR_ORDER = 1
        CEN_PIX  = 396
        WAVEBAND = 2
    LL_IND   = 3
        LINENAME = Ne VI
        WAVELNTH = 562.803
        GR_ORDER = 1
        CEN_PIX  = 439
        WAVEBAND = 2
    LL_IND   = 4
        LINENAME = He I
        WAVELNTH = 584.33
        GR_ORDER = 1
        CEN_PIX  = 623
        WAVEBAND = 2
    LL_IND   = 5
        LINENAME = Mg X
        WAVELNTH = 624.941
        GR_ORDER = 1
        CEN_PIX  = 969
        WAVEBAND = 2
    LL_IND   = 6
        LINENAME = O V
        WAVELNTH = 629.153
        GR_ORDER = 1
        CEN_PIX  = 1005
        WAVEBAND = 2

DATAWIN
    DW_ID    = 571
    DETECTOR = N
    DW_DESC  = Background,   6 lines. {0}  dex = (37,90) pixels <22805>
    W_WIDTH  = 37
    W_HEIGHT = 90
    VDS_BACK = 1
    LL_ID    = 440
    N_WINS   = 10
    DW_IND   = 1
        WIN_NAME = O_4_554_52                              
        WIN_DEF  = (350,407,37,90)
        WIN_FLAG = 0
    DW_IND   = 2
        WIN_NAME = Ca_10_557_77                            
        WIN_DEF  = (378,407,37,90)
        WIN_FLAG = 0
    DW_IND   = 3
        WIN_NAME = Ne_6_562_80                             
        WIN_DEF  = (421,407,37,90)
        WIN_FLAG = 0
    DW_IND   = 4
        WIN_NAME = He_1_584_33                             
        WIN_DEF  = (605,407,37,90)
        WIN_FLAG = 0
    DW_IND   = 5
        WIN_NAME = Mg_10_624_94                            
        WIN_DEF  = (951,407,37,90)
        WIN_FLAG = 0
    DW_IND   = 6
        WIN_NAME = O_5_629_15                              
        WIN_DEF  = (987,407,36,90)
        WIN_FLAG = 0
    DW_IND   = 7
        WIN_NAME = Background                              
        WIN_DEF  = (20,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 8
        WIN_NAME = Background                              
        WIN_DEF  = (994,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 9
        WIN_NAME = Background                              
        WIN_DEF  = (20,994,10,10)
        WIN_FLAG = 0
    DW_IND   = 10
        WIN_NAME = Background                              
        WIN_DEF  = (994,994,10,10)
        WIN_FLAG = 0

RASTER
    RAS_ID   = 160
    DETECTOR = N
    RAS_DESC = Slit(4x240),Posns(250,-)@(0,-) steps
    SLIT_NUM = 5
    XSTEP    = 0
    YSTEP    = 0
    NX       = 250
    NY       = 1

RASTER_VAR
    RAS_ID   = 160
    RAS_VAR  = 12
    RV_DESC  = (4x180) arcsec, 15s <ACTIVE>  Comp. (8,2) IDs-(440,571)
    EXPTIME  = 15
    LL_ID    = 440
    COMP_ID  = 8
    COMP_OPT = 2
    DW_ID    = 571
    IEF_ID   = 0
    VDS_ORIENT = 0
    VDS_MAP  = 2
    TEL_RATE = M
    DURATION = 5051
    USABLE   = Y

STUDY
    STUDY_ID = 194
    TITLE_ID = 385
    OBS_PROG = SAS250W
    TITLE    = TIME SERIES, 250 REP, 4X240 SLIT
    CATEGORY = S
    VAR_POINT = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 160
        POINTING = 1
        INS_X    = 0
        INS_Y    = 0

STUDY_VAR
    STUDY_ID = 194
    TITLE_ID = 385
    STUDYVAR = 12
    SV_DESC  = 15 S, 4''X180'' AREA, SUM 2 ROWS, TR+UPPER TR
    N_RASTERS0 = 0
    DURATION0 = 0
    DURATION1 = 5051
    ZONE_ID  = 5
    USABLE   = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 160
        RAS_VAR  = 12
        N_REPEAT_R = 1
