DATATYPE = CDS STUDY DEFINITION
FILENAME = /eofcs/data/plan/database/export/merc1_14.def
INSTRUME = CDS
DATE_CRE = 1999/10/08 19:01:04
END

LINELIST
    LL_ID    = 331
    DETECTOR = N
    LL_DESC  = Mercury fast-step observation line list
    N_LINES  = 7
    LL_IND   = 1
        LINENAME = Cont_2
        WAVELNTH = 531
        GR_ORDER = 1
        CEN_PIX  = 166
        WAVEBAND = 2
    LL_IND   = 2
        LINENAME = Cont_1
        WAVELNTH = 330.61
        GR_ORDER = 1
        CEN_PIX  = 335
        WAVEBAND = 1
    LL_IND   = 3
        LINENAME = O IV
        WAVELNTH = 554.8
        GR_ORDER = 1
        CEN_PIX  = 370
        WAVEBAND = 2
    LL_IND   = 4
        LINENAME = O III
        WAVELNTH = 600
        GR_ORDER = 1
        CEN_PIX  = 757
        WAVEBAND = 2
    LL_IND   = 5
        LINENAME = Fe XII
        WAVELNTH = 364.493
        GR_ORDER = 1
        CEN_PIX  = 817
        WAVEBAND = 1
    LL_IND   = 6
        LINENAME = Mg X
        WAVELNTH = 625.3
        GR_ORDER = 1
        CEN_PIX  = 972
        WAVEBAND = 2
    LL_IND   = 7
        LINENAME = O V
        WAVELNTH = 629.741
        GR_ORDER = 1
        CEN_PIX  = 1010
        WAVEBAND = 2

DATAWIN
    DW_ID    = 434
    DETECTOR = N
    DW_DESC  = Background,   7 lines. {0}  dex = (35,30) pixels <29370>
    W_WIDTH  = 35
    W_HEIGHT = 30
    VDS_BACK = 1
    LL_ID    = 331
    N_WINS   = 11
    DW_IND   = 1
        WIN_NAME = WW_531_00                               
        WIN_DEF  = (149,437,35,30)
        WIN_FLAG = 0
    DW_IND   = 2
        WIN_NAME = WW_330_61                               
        WIN_DEF  = (318,557,35,30)
        WIN_FLAG = 0
    DW_IND   = 3
        WIN_NAME = O_4_554_80                              
        WIN_DEF  = (353,437,35,30)
        WIN_FLAG = 0
    DW_IND   = 4
        WIN_NAME = O_3_600_00                              
        WIN_DEF  = (740,437,35,30)
        WIN_FLAG = 0
    DW_IND   = 5
        WIN_NAME = Fe_12_364_49                            
        WIN_DEF  = (800,557,35,30)
        WIN_FLAG = 0
    DW_IND   = 6
        WIN_NAME = Mg_10_625_30                            
        WIN_DEF  = (955,437,35,30)
        WIN_FLAG = 0
    DW_IND   = 7
        WIN_NAME = O_5_629_74                              
        WIN_DEF  = (993,437,30,30)
        WIN_FLAG = 0
    DW_IND   = 8
        WIN_NAME = Background                              
        WIN_DEF  = (20,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 9
        WIN_NAME = Background                              
        WIN_DEF  = (994,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 10
        WIN_NAME = Background                              
        WIN_DEF  = (20,994,10,10)
        WIN_FLAG = 0
    DW_IND   = 11
        WIN_NAME = Background                              
        WIN_DEF  = (994,994,10,10)
        WIN_FLAG = 0

RASTER
    RAS_ID   = 71
    DETECTOR = N
    RAS_DESC = Slit(4x240),Posns(10,-)@(4,-) steps
    SLIT_NUM = 5
    XSTEP    = 4
    YSTEP    = 0
    NX       = 10
    NY       = 1

RASTER_VAR
    RAS_ID   = 71
    RAS_VAR  = 24
    RV_DESC  = (40x60) arcsec, 6.7s <QUIET>  Comp. 2 IDs-(331,434)
    EXPTIME  = 6.7
    LL_ID    = 331
    COMP_ID  = 2
    COMP_OPT = 0
    DW_ID    = 434
    IEF_ID   = 0
    VDS_ORIENT = 0
    VDS_MAP  = 2
    TEL_RATE = M
    DURATION = 106
    USABLE   = Y

STUDY
    STUDY_ID = 104
    TITLE_ID = 446
    OBS_PROG = MERC1
    TITLE    = MERCURY 1
    CATEGORY = S
    VAR_POINT = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 71
        POINTING = 1
        INS_X    = 0
        INS_Y    = 0

STUDY_VAR
    STUDY_ID = 104
    TITLE_ID = 446
    STUDYVAR = 14
    SV_DESC  = V 1
    N_RASTERS0 = 0
    DURATION0 = 0
    DURATION1 = 106
    ZONE_ID  = 1
    USABLE   = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 71
        RAS_VAR  = 24
        N_REPEAT_R = 1
