DATATYPE = CDS STUDY DEFINITION
FILENAME = /eofcs/data/plan/database/export/pobs1_2_18.def
INSTRUME = CDS
DATE_CRE = 1997/05/20 15:31:53
END

LINELIST
    LL_ID    = 182
    DETECTOR = N
    LL_DESC  = jop 12, may 1997
    N_LINES  = 15
    LL_IND   = 1
        LINENAME = O III
        WAVELNTH = 525.8
        GR_ORDER = 1
        CEN_PIX  = 109
        WAVEBAND = 2
    LL_IND   = 2
        LINENAME = Si XII
        WAVELNTH = 320.66
        GR_ORDER = 1
        CEN_PIX  = 187
        WAVEBAND = 1
    LL_IND   = 3
        LINENAME = He I
        WAVELNTH = 537.03
        GR_ORDER = 1
        CEN_PIX  = 205
        WAVEBAND = 2
    LL_IND   = 4
        LINENAME = O IV
        WAVELNTH = 553.33
        GR_ORDER = 1
        CEN_PIX  = 345
        WAVEBAND = 2
    LL_IND   = 5
        LINENAME = O IV
        WAVELNTH = 554.52
        GR_ORDER = 1
        CEN_PIX  = 355
        WAVEBAND = 2
    LL_IND   = 6
        LINENAME = Ca X
        WAVELNTH = 557.77
        GR_ORDER = 1
        CEN_PIX  = 383
        WAVEBAND = 2
    LL_IND   = 7
        LINENAME = Ne VI
        WAVELNTH = 562.83
        GR_ORDER = 1
        CEN_PIX  = 427
        WAVEBAND = 2
    LL_IND   = 8
        LINENAME = Si IX
        WAVELNTH = 345.13
        GR_ORDER = 1
        CEN_PIX  = 536
        WAVEBAND = 1
    LL_IND   = 9
        LINENAME = Fe XIII
        WAVELNTH = 348.18
        GR_ORDER = 1
        CEN_PIX  = 580
        WAVEBAND = 1
    LL_IND   = 10
        LINENAME = He I
        WAVELNTH = 584.33
        GR_ORDER = 1
        CEN_PIX  = 610
        WAVEBAND = 2
    LL_IND   = 11
        LINENAME = O III
        WAVELNTH = 599.59
        GR_ORDER = 1
        CEN_PIX  = 740
        WAVEBAND = 2
    LL_IND   = 12
        LINENAME = He II
        WAVELNTH = 303.78
        GR_ORDER = 2
        CEN_PIX  = 808
        WAVEBAND = 2
    LL_IND   = 13
        LINENAME = Mg IX
        WAVELNTH = 368.068
        GR_ORDER = 1
        CEN_PIX  = 862
        WAVEBAND = 1
    LL_IND   = 14
        LINENAME = Mg X
        WAVELNTH = 624.94
        GR_ORDER = 1
        CEN_PIX  = 956
        WAVEBAND = 2
    LL_IND   = 15
        LINENAME = O V
        WAVELNTH = 629.73
        GR_ORDER = 1
        CEN_PIX  = 997
        WAVEBAND = 2

DATAWIN
    DW_ID    = 245
    DETECTOR = N
    DW_DESC  = Background,  15 lines. {0}  dex = (21,120) pixels <20561>
    W_WIDTH  = 21
    W_HEIGHT = 120
    VDS_BACK = 1
    LL_ID    = 182
    N_WINS   = 19
    DW_IND   = 1
        WIN_NAME = O_3_525_80                              
        WIN_DEF  = (99,392,21,120)
        WIN_FLAG = 0
    DW_IND   = 2
        WIN_NAME = Si_12_320_66                            
        WIN_DEF  = (177,512,21,120)
        WIN_FLAG = 0
    DW_IND   = 3
        WIN_NAME = He_1_537_03                             
        WIN_DEF  = (195,392,21,120)
        WIN_FLAG = 0
    DW_IND   = 4
        WIN_NAME = O_4_553_33                              
        WIN_DEF  = (335,392,21,120)
        WIN_FLAG = 0
    DW_IND   = 5
        WIN_NAME = O_4_554_52                              
        WIN_DEF  = (345,392,21,120)
        WIN_FLAG = 0
    DW_IND   = 6
        WIN_NAME = Ca_10_557_77                            
        WIN_DEF  = (373,392,21,120)
        WIN_FLAG = 0
    DW_IND   = 7
        WIN_NAME = Ne_6_562_83                             
        WIN_DEF  = (417,392,21,120)
        WIN_FLAG = 0
    DW_IND   = 8
        WIN_NAME = Si_9_345_13                             
        WIN_DEF  = (526,512,21,120)
        WIN_FLAG = 0
    DW_IND   = 9
        WIN_NAME = Fe_13_348_18                            
        WIN_DEF  = (570,512,21,120)
        WIN_FLAG = 0
    DW_IND   = 10
        WIN_NAME = He_1_584_33                             
        WIN_DEF  = (600,392,21,120)
        WIN_FLAG = 0
    DW_IND   = 11
        WIN_NAME = O_3_599_59                              
        WIN_DEF  = (730,392,21,120)
        WIN_FLAG = 0
    DW_IND   = 12
        WIN_NAME = He_2_303_78                             
        WIN_DEF  = (798,392,21,120)
        WIN_FLAG = 0
    DW_IND   = 13
        WIN_NAME = Mg_9_368_07                             
        WIN_DEF  = (852,512,21,120)
        WIN_FLAG = 0
    DW_IND   = 14
        WIN_NAME = Mg_10_624_94                            
        WIN_DEF  = (946,392,21,120)
        WIN_FLAG = 0
    DW_IND   = 15
        WIN_NAME = O_5_629_73                              
        WIN_DEF  = (987,392,21,120)
        WIN_FLAG = 0
    DW_IND   = 16
        WIN_NAME = Background                              
        WIN_DEF  = (20,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 17
        WIN_NAME = Background                              
        WIN_DEF  = (994,20,10,10)
        WIN_FLAG = 0
    DW_IND   = 18
        WIN_NAME = Background                              
        WIN_DEF  = (20,994,10,10)
        WIN_FLAG = 0
    DW_IND   = 19
        WIN_NAME = Background                              
        WIN_DEF  = (994,994,10,10)
        WIN_FLAG = 0

RASTER
    RAS_ID   = 38
    DETECTOR = N
    RAS_DESC = Slit(4x240),Posns(30,-)@(4,-) steps
    SLIT_NUM = 5
    XSTEP    = 4
    YSTEP    = 0
    NX       = 30
    NY       = 1

RASTER_VAR
    RAS_ID   = 38
    RAS_VAR  = 18
    RV_DESC  = (120x240) arcsec, 100s <QUIET>  Comp. 2 IDs-(182,245)
    EXPTIME  = 100
    LL_ID    = 182
    COMP_ID  = 2
    COMP_OPT = 0
    DW_ID    = 245
    IEF_ID   = 0
    VDS_ORIENT = 0
    VDS_MAP  = 2
    TEL_RATE = M
    DURATION = 3179
    USABLE   = Y

STUDY
    STUDY_ID = 44
    TITLE_ID = 64
    OBS_PROG = POBS1_2
    TITLE    = PROMINENCE OBS PROGRAMME 1 PART 2
    CATEGORY = S
    VAR_POINT = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 38
        POINTING = 1
        INS_X    = 0
        INS_Y    = 0

STUDY_VAR
    STUDY_ID = 44
    TITLE_ID = 64
    STUDYVAR = 18
    SV_DESC  = JOP 12, MAY 1997
    N_RASTERS0 = 0
    DURATION0 = 0
    DURATION1 = 3179
    ZONE_ID  = 4
    USABLE   = Y
    N_RASTER_DEF = 1
    RAS_IND   = 1
        RAS_ID   = 38
        RAS_VAR  = 18
        N_REPEAT_R = 1
